THEN PLACES IT IN OTHER CONTAINER

STOP

THE CONTAINER COMES OUT OF THE C-BELT

ROBOTIC ARM TRAVELS TO THE C-BELT AND PICKS THE PLANT

START